ITB #7139-09-ELD, LP&L 6 and 12 Yard Dump Trucks

	SUBMIT TO:

LUBBOCK POWER & LIGHT

PURCHASING DEPARTMENT

402 MUNICIPAL DRIVE

LUBBOCK, TX 79403-3302
	
[image: image1.png]


         
AN EQUAL

OPPORTUNITY                
EMPLOYER

	Ron Shuffield

Purchasing Manager Electric Utilities
	

	TEL: 806.775.2170

FAX: 806.775.3590

http://rshuffield@mylubbock.us
	

	TITLE:

LP&L 6 and 12 Yard Dump Trucks
	SUBMITTAL DEADLINE:

September 2, 2009, 2:00 P. M. CST

	PRE BID DATE, TIME AND LOCATION: 

DELETED
	Any bids received after the time and date listed above, regardless of the mode of delivery, shall be returned unopened.

	RESPONDENT NAME:


	LABEL THE OUTSIDE OF YOUR SEALED BID WITH THE ITB NUMBER, THE CLOSING DATE AND TIME, AND YOUR COMPANY NAME AND ADDRESS.
IF RETURNING AS A “NO BID”, PLEASE COMPLETE AND RETURN THE “STATEMENT OF NO BID”.

	MAILING ADDRESS:


	

	CITY – STATE – ZIP:


	LUBBOCK POWER & LIGHT RESERVES THE RIGHT TO ACCEPT OR REJECT ANY AND ALL BIDS IN WHOLE OR IN PART AND WAIVE ANY INFORMALITY IN THE COMPETITIVE BID PROCESS.  FURTHER, LP&L RESERVES THE RIGHT TO ENTER INTO ANY CONTRACT DEEMED TO BE IN THE BEST INTEREST OF LP&L. 

IT IS THE INTENT AND PURPOSE OF LUBBOCK POWER & LIGHT THAT THIS REQUEST PERMITS COMPETITIVE BIDS.  IT IS THE BIDDER’S RESPONSIBILITY TO ADVISE THE LUBBOCK POWER & LIGHT PURCHASING MANAGER IF ANY LANGUAGE, REQUIREMENTS, ETC., OR ANY COMBINATIONS THEREOF, INADVERTENTLY RESTRICTS OR LIMITS THE REQUIREMENTS STATED IN THIS ITB TO A SINGLE SOURCE.  SUCH NOTIFICATION MUST BE SUBMITTED IN WRITING AND MUST BE RECEIVED BY THE PURCHASING MANAGER NO LATER THAN FIVE (5) BUSINESS DAYS PRIOR TO THE ABOVE SUBMITTAL DEADLINE.  

	TELEPHONE NO:


	

	FAX NO:


	

	E-MAIL:


	

	FEDERAL TAX ID NO. OR SOCIAL SECURITY NO.


	


THE BIDDER HEREBY ACKNOWLEDGES RECEIPT OF AND AGREES ITS BID IS BASED ON ANY ADDENDA POSTED ON RFPDEPOT.COM
An officer or employee of Lubbock Power & Light cannot benefit from any contract, job, work or service for the utility or be interested in the sale to Lubbock Power & Light of any supplies, equipment, material or articles purchased.  Will any officer or employee of Lubbock Power & Light, or member of their immediate family, benefit from the award of this bid to the above firm?
 YES
 NO

IN COMPLIANCE WITH THIS SOLICITATION, THE UNDERSIGNED BIDDER HAVING EXAMINED THE INVITATION TO BID AND SPECIFICATIONS, AND BEING FAMILIAR WITH THE CONDITIONS TO BE MET, HEREBY SUBMITS THE FOLLOWING BID FOR FURNISHING THE MATERIAL, EQUIPMENT, LABOR AND EVERYTHING NECESSARY FOR PROVIDING THE ITEMS LISTED ON THE ATTACHED BID FORM AND AGREES TO DELIVER SAID ITEMS AT THE LOCATIONS AND FOR THE PRICES SET FORTH ON THE BID FORM.  AN INDIVIDUAL AUTHORIZED TO BIND THE COMPANY MUST SIGN THE FOLLOWING SECTION.  FAILURE TO EXECUTE THIS PORTION MAY RESULT IN BID REJECTION.

By my signature I certify that this offer is made without prior understanding, agreement, or connection with any corporation, firm, business entity, or person submitting an offer for the same materials, supplies, equipment, or service(s), and is in all respects fair and without collusion or fraud. I further agree that if the offer is accepted, the offeror will convey, sell, assign, or transfer to Lubbock Power & Light all right, title, and interest in and to all causes of action it may now or hereafter acquire under the Anti-trust laws of the United States and the State of Texas for price fixing relating to the particular commodity(s) or service (s) purchased or acquired by Lubbock Power & Light. At Lubbock Power & Light’s discretion, such assignment shall be made and become effective at the time Lubbock Power & Light tenders final payment to the vendor.

Authorized Signature




Title

Print/Type Name





Date
THIS FORM MUST BE COMPLETED AND RETURNED WITH YOUR RESPONSE.
BID FORM

LP&L 6 and 12 Yard Dump Trucks
CITY OF LUBBOCK, TEXAS

ITB #7139-09-ELD

In compliance with the Invitation to Bid #7139-09-ELD, the undersigned Bidder having examined the Invitation to Bid and Specifications, and being familiar with the conditions to be met, hereby submits the following Bid for furnishing the material, equipment, labor and everything necessary for providing the items listed below and agrees to deliver said items at the locations and for the prices set forth on this form.  The Invitation to Bid #7139-09-ELD is by reference incorporated in this contract. The Bid Form must be completed in blue or black ink or by typewriter.
	ITEM
	QTY
	Unit

of

Measure
	DESCRIPTION
	UNIT PRICE* BID
	EXTENDED COST
	Delivery (Days)

After Receipt of Order
	One Set of Mfr’s Repair, Parts & Service Manuals (hard copy & CD)

	1.
	1
	Each
	6 Yard Dump Truck with Hydraulic Hoist Per Spec7313-100
	$
	$
	
	$

	
	
	
	OEM manufacturer’s OEM EXTENDED WARRANTY SHALL INCLUDE THE COMPLETE CHASSIS, ENGINE AND OEM ATTACHED COMPONENTS, RADIATOR, FAN CLUTCH, IDLER PULLEYS, TRANSMISSION, AND SELECTOR CONTROLS, DRIVELINES AND U-JOINTS, ELECTRICAL SYSTEM INCLUDING OEM WIRE HARNESS, ALTERNATOR, STARTER, DASH INSTRUMENTATION AND CONTROLS, FULL SUSPENSION, STEERING, COMPUTERS SYSTEM.  WARRANTY SHALL INCLUDE 7000 HOURS,  FIVE (5) YEARS, 100,000 MILES no DEDUCTIBLE.                                                                                                        
	
	
	

	
	
	
	Brand Name and Model Number:

	2.
	1
	Each
	12 Yard Dump Truck  with Hydraulic Hoist Per Spec 7412-722
	$
	$
	
	$

	
	
	
	OEM manufacturer’s OEM EXTENDED WARRANTY SHALL INCLUDE THE COMPLETE CHASSIS, ENGINE AND OEM ATTACHED COMPONENTS, RADIATOR, FAN CLUTCH, IDLER PULLEYS, TRANSMISSION, AND SELECTOR CONTROLS, DRIVELINES AND U-JOINTS, ELECTRICAL SYSTEM INCLUDING OEM WIRE HARNESS, ALTERNATOR, STARTER, DASH INSTRUMENTATION AND CONTROLS, FULL SUSPENSION, STEERING, COMPUTERS SYSTEM.  WARRANTY SHALL INCLUDE 7000 HOURS, FIVE (5) YEARS, 100,000 MILES no DEDUCTIBLE.                                                                                                  
	
	
	

	
	
	
	Brand Name and Model Number:


*PRICE: F.O.B. Lubbock Power & Light, 404 Municipal Drive - Lubbock, Texas

PAYMENT TERMS AND DISCOUNTS - Bidder offers a prompt payment discount of 

%, net 
 calendar days. Discounts will not be considered in determining low bid.  Unless otherwise indicated on the Bid Form, payment terms will be NET THIRTY DAYS.  LP&L will pay the successful bidder within thirty days after the receipt of a correct invoice or after the date of acceptance, whichever event occurs later.  Discounts for prompt payment requiring payment by LP&L within a stipulated number of days will be interpreted as applying within the stipulated number of calendar days after the date of receipt by LP&L of a correct invoice or after the date of acceptance that meets contract requirements, whichever event occurs later.  Discounts for payment in less than ten days will not be considered.

THIS BID IS SUBMITTED BY 



a corporation organized under the laws of the State of ____________________, or a partnership consisting of 




 or individual trading as _______________________________________________ of the City of 






Firm:













Address:












City:






 State:


 Zip




	M/WBE Firm:
	
	Woman
	
	Black American
	
	Native American

	
	
	Hispanic American
	
	Asian Pacific American
	
	Other (Specify)


Any entity or person that manufactures, distributes, converts new motor vehicles (or represents an entity that manufactures, distributes, or converts new motor vehicles) or is in the business of buying, exchanging, or selling new motor vehicles is required under the Tex. Occ. Code. Chapter 2301 to be licensed by Motor Vehicle Division of the Texas Department of Transportation.  In order for a bid to be in compliance with the Motor Vehicle Commission Code, the bidder must hold and provide all applicable current valid licenses issued by the State of Texas:

1. Name



 and Manufacture’s License No.





2. Name



 and Converter’s License No.





3. Name



 and Representative’s License No.





4. Name



 and Franchise Dealer’s License No.




General Distinguishing No.




 (Franchised TX dealer)

By








Date:




Authorized Representative - must sign by hand
Officer Name and Title:












Please Print
Business Telephone Number





  FAX:





FOR LP&L USE ONLY
Bid Form Item Number(s) Awarded to Above Named Firm/Individual:





 

Date of Award by ____________________________________Date P.O./Contract Issued:_____________________

RETURN COMPLETED & SIGNED BID FORM ALONG WITH LUBBOCK POWER & LIGHT SPECIFICATIONS.

LABEL THE OUTSIDE OF YOUR SEALED BID WITH THE ITB NUMBER, THE CLOSING DATE AND TIME, AND YOUR COMPANY NAME AND ADDRESS.

LP&L 6 and 12 Yard Dump Trucks
LUBBOCK POWER & LIGHT

ITB #7139-09-ELD


LUBBOCK POWER & LIGHT APPRECIATES YOUR TIME AND EFFORT IN PREPARING YOUR BID.  ALL BIDDERS SHOULD FAMILIARIZE THEMSELVES WITH THE FOLLOWING INSTRUCTIONS TO BIDDERS, GENERAL CONDITIONS, AND ATTACHED SPECIFICATIONS.

I. INSTRUCTIONS TO BIDDERS

1
Bid Delivery, Time & Date
1.1
Lubbock Power & Light is seeking written and sealed competitive bids to furnish LP&L 6 and 12 Yard Dump Trucks per the attached specifications.  Sealed bids will be received no later than 2:00 p.m. CST, September 2, 2009, if date/time stamped on or before 2:00 p.m. at the office listed below.  Any bid received after the date and hour specified will be rejected and returned unopened to the bidder.  EACH BID AND SUPPORTING DOCUMENTATION MUST BE IN A SEALED ENVELOPE OR CONTAINER PLAINLY LABELED IN THE LOWER LEFT-HAND CORNER:  "ITB #7139-09-ELD, LP&L 6 AND 12 YARD DUMP TRUCKS" AND THE BID OPENING DATE AND TIME.  BIDDERS MUST ALSO INCLUDE THEIR COMPANY NAME AND ADDRESS ON THE OUTSIDE OF THE ENVELOPE OR CONTAINER.  Bids must be addressed to:

Ron Shuffield, Purchasing Manager Electric Utilities

Lubbock Power & Light

402 Municipal Drive

Lubbock, Texas 79403

1.2
Bidders are responsible for making certain bids are delivered to the Purchasing Department.  Mailing of a bid does not ensure that the bid will be delivered on time or delivered at all.  If bidder does not hand deliver bid, we suggest that he/she use some sort of delivery service that provides a receipt. Lubbock Power & Light assumes no responsibility for errant delivery of bids, including those relegated to a courier agent who fails to deliver in accordance with the time and receiving point specified.

1.3
Bids will be accepted in person, by United States Mail, by United Parcel Service, or by private courier service.  No bids will be accepted by oral communication, telephone, electronic mail, telegraphic transmission, or telefacsimile transmission.  Lubbock Power & Light WILL NOT ACCEPT FAX BIDS. The Bid Form must be completed in blue or black ink or by typewriter.
1.4
Bids may be withdrawn prior to the above scheduled time set for closing of the bids. Bids CANNOT be withdrawn, altered or amended after bid closing.  Alteration made before bid closing must be initiated by bidder guaranteeing authenticity. 

1.5
Lubbock Power & Light reserves the right to postpone the date and time for opening bids through an addendum.

2
Pre-bid meeting--deleted
3
CLARIFICATION OF REQUIREMENTS
3.1
It is the intent and purpose of Lubbock Power & Light that this request permits competitive bids.  It is the bidder’s responsibility to advise the Lubbock Power & Light Purchasing Manager if any language, requirements, etc., or any combinations thereof, inadvertently restricts or limits the requirements stated in this ITB to a single source.  Such notification must be submitted in writing and must be received by the Purchasing Manager no later than five (5) business days prior to the bid closing date.  A review of such notifications will be made.

3.2
ALL REQUESTS FOR ADDITIONAL INFORMATION OR CLARIFICATION CONCERNING THIS INVITATION TO BID (ITB) MUST BE SUBMITTED IN WRITING NO LATER THAN FIVE (5) BUSINESS DAYS PRIOR TO THE BID CLOSING DATE AND ADDRESSED TO: 

Ron Shuffield, Purchasing Manager Electric Utilities

Lubbock Power & Light

402 Municipal Drive

Lubbock, Texas 79403

Fax:
(806) 775-3590

4
Addenda & Modifications
4.1
Any changes, additions, or clarifications to the ITB are made by ADDENDA information available over the Internet atpublic librarieshttp://www.BidSync.com

. We strongly suggest that you check for any addenda a minimum of forty-eight hours in advance of the response deadline. BUSINESSES WITHOUT INTERNET ACCESS may use computers available at most  . 
4.2
Any offeror in doubt as to the true meaning of any part of the ITB or other documents may request an interpretation thereof from the Purchasing Manager. At the request of the offeror, or in the event the Purchasing Manager deems the interpretation to be substantive, the interpretation will be made by written addenda issued by the Purchasing Manager. Such addenda issued by the Purchasing Manager will be available over the Internet athttp://www.BidSync.com  and will become part of the proposal package having the same binding effect as provisions of the original ITB.  No verbal explanations or interpretations will be binding. In order to have a request for interpretation considered, the request must be submitted in writing and must be received by Lubbock Power & Light.

4.3
All addenda, amendments, and interpretations of this solicitation shall be in writing.  Lubbock Power & Light shall not be legally bound by any amendment or interpretation that is not in writing.  Only information supplied by Lubbock Power & Light in writing or in this ITB should be used in preparing bid responses.  All contacts that a bidder may have had before or after receipt of this ITB with any individuals, employees, or representatives of Lubbock Power & Light and any information that may have been read in any news media or seen or heard in any communication facility regarding this bid should be disregarded in preparing responses.

4.4 Lubbock Power & Light does not assume responsibility for the receipt of any addendum sent to bidders.

5
Examination of Documents and REQUIREMENTS
5.1
Each bidder shall carefully examine all ITB documents and thoroughly familiarize itself with all requirements prior to submitting a bid to ensure that the goods and/or services being bid meet the intent of these specifications.

5.2
Before submitting a bid, each bidder shall be responsible for making all investigations and examinations that are necessary to ascertain conditions and requirements affecting the requirements of this Invitation to Bid.  Failure to make such investigations and examinations shall not relieve the bidder from obligation to comply, in every detail, with all provisions and requirements of the Invitation to Bid.

6
Bid SUBMITTAL
6.1
BIDDERS MUST SUBMIT THE ORIGINAL AND ONE COPY OF THE SEALED BID TO THE PURCHASING DEPARTMENT PRIOR TO RESPONSE DUE DATE/TIME.  FAILURE TO SUBMIT THE ADDITIONAL COPY MAY RESULT IN THE BID BEING DECLARED UNRESPONSIVE TO SPECIFICATION AND MAY NOT BE FURTHER EVALUATED.  The original must be clearly marked “ORIGINAL” and the copy must be clearly marked “COPY”.
6.2
Bids must be submitted on the Bid Form and the Bidder must sign and date their bid in the space provided.  Identify the item bid, including brand name and model number, if applicable.  Enter unit price, extended cost, and delivery days in the columns provided.  In the event of discrepancies in extension, the unit price shall govern. THE BID FORM MUST BE COMPLETED IN BLUE OR BLACK INK OR BY TYPEWRITER.
6.3
Lubbock Power & Light is exempt from Federal Excise, State Sales and Transportation taxes.  TAX MUST NOT BE INCLUDED IN BID.  Tax exemption certificates will be executed by the Purchasing Manager upon request.

6.4
Any information regarding warranties and/or maintenance agreements pertaining to said bid item(s) are to be included in the bid.

6.5
Bids will not be considered unless bid F.O.B. delivered and include all delivery and packaging costs.  The number of calendar days required to place the materials in Lubbock Power & Light’s receiving point under normal conditions must be shown on the Bid Form.  DO NOT quote shipping dates.  Failure to indicate delivery days on the Bid Form will obligate Bidder to complete delivery in two weeks.  A minimum of five days better delivery will automatically break a tie bid.  Unrealistically short or undue long delivery promises may cause bid to be disregarded.  Consistent failure of a bidder to meet delivery promises without a valid reason may cause removal from the bid list. 

6.6
Bid prices must be firm for a minimum period of sixty (60) days.  Bids subject to price increases will not be considered. 

6.7 All bids, responses, inquiries, or correspondence relating to or in reference to this ITB, and all reports, charts, and other documentation submitted by bidders shall become the property of Lubbock Power & Light when received.

6.8 If there are any additional charges of any kind, other than those mentioned above, specified or unspecified, offeror MUST indicate the items required and attendant costs or forfeit the right to payment for such items.

6.9 LABEL THE OUTSIDE OF YOUR SEALED BID WITH THE ITB NUMBER, THE CLOSING DATE AND TIME, AND YOUR COMPANY NAME AND ADDRESS.

7
Bid Preparation Costs
7.1
Issuance of this ITB does not commit Lubbock Power & Light, in any way, to pay any costs incurred in the preparation and submission of a bid.  Also, should a bidder bid an alternate, any test costs to prove equality of product will be at the expense of the bidder, not Lubbock Power & Light.

7.2
The issuance of this ITB does not obligate Lubbock Power & Light to enter into contract for any services or equipment.

7.3 All costs related to the preparation and submission of a bid shall be paid by the bidder.

8
TRADE SECRETS, CONFIDENTIAL INFORMATION AND THE TEXAS PUBLIC INFORMATION ACT
8.1
If you consider any portion of your bid to be privileged or confidential by statute or judicial decision, including trade secrets and commercial or financial information, clearly identify those portions. 

8.2
Lubbock Power & Light will honor your notations of trade secrets and confidential information and decline to release such information initially, but please note that the final determination of whether a particular portion of your bid is in fact a trade secret or commercial or financial information that may be withheld from public inspection will be made by the Texas Attorney General or a court of competent jurisdiction.  In the event a public information request is received for a portion of your bid that you have marked as being confidential information, you will be notified of such request and you will be required to justify your legal position in writing to the Texas Attorney General pursuant to Section 552.305 of the Government Code.  In the event that it is determined by opinion or order of the Texas Attorney General or a court of competent jurisdiction that such information is in fact not privileged and confidential under Section 552.110 of the Government Code and Section 252.049 of the Local Government Code, then such information will be made available to the requester.

8.3
Marking your entire bid CONFIDENTIAL/PROPRIETARY is not in conformance with the Texas Open Records Act.

9
LICENSES, PERMITS, Taxes 

9.1
The price or prices for the work shall include full compensation for all taxes, permits, etc. that the bidder is or may be required to pay.

10
Historically Underutilized Business (HUB) Requirements
10.1
Lubbock Power & Light hereby notifies all bidders that in regard to any contract entered into pursuant to this ITB, Historically Underutilized Businesses (HUB's) will be afforded equal opportunities to submit bids and will not be discriminated against on the grounds of race, color, sex, disability, or national origin in consideration of an award.

10.2
A HUB is defined as a small business concern which is at least 51% owned and controlled by one or more socially and economically disadvantaged individuals, or in the case of any publicly owned business, at least 51% of the stock of which is owned by one ore more socially and economically disadvantaged individuals.  Socially and economically disadvantaged include Women, Black Americans, Hispanic Americans, Native Americans, Asian-Pacific Americans, and Asian-Indian Americans.

11
CONFLICT OF INTEREST
11.1
The bidder shall not offer or accept gifts or anything of value nor enter into any business arrangement with any employee, official or agent of the Lubbock Power & Light.

11.2.1 By signing and executing this bid, the bidder certifies and represents to Lubbock Power & Light the bidder has not offered, conferred or agreed to confer any pecuniary benefit or other thing of value for the receipt of special treatment, advantage, information, recipient's decision, opinion, recommendation, vote or any other exercise of discretion concerning this bid.  

12
Authorization to Bind Submitter of Bid
12.1
Bids must show vendor name and address of bidder.  Bids must be manually signed by an officer of the company authorized to bind the submitter to its provisions.  Person signing bid must show title or AUTHORITY TO BIND THEIR FIRM IN A CONTRACT. Failure to manually sign bid will disqualify it.  

12.2
The bid submitted by the bidder shall become an integral part of the contract between Lubbock Power & Light and the Bidder and the representations, covenants, and conditions therein contained shall be binding upon the person, firm or corporation executing the same.

13
BID Award
13.1 The contract may be awarded either to the lowest responsible bidder or to the bidder who provides goods or services at the best value for Lubbock Power & Light. In determining the best value for the Lubbock Power & Light, the Lubbock Power & Light may consider:

a)
The purchase price;

b)
The reputation of the of the bidder and of the bidder’s goods or services;

c)
The quality of the bidder’s goods or services;

d)
The extent to which the goods or services meet Lubbock Power & Light’s needs;

e)
The bidder’s past relationship with Lubbock Power & Light;

f)
The impact on the ability of LP&L to comply with laws and rules relating to contracting with Historically Underutilized Businesses and non-profit organizations employing persons with disabilities;

g)
The total long-term cost to LP&L to acquire goods or services; and

h)
Any relevant criteria specifically listed in the Invitation to Bid.

13.2 Lubbock Power & Light reserves the right to reject any or all bids, reject any particular item on a bid, and to waive immaterial formalities and to accept the offer most advantageous to the Lubbock Power & Light in its sole discretion.  Unless otherwise specified herein, Lubbock Power & Light may award the bid for any item or group of items shown on the Bid Form.

13.3 All bids are evaluated for compliance with specifications before the bid price is considered. Failure to comply with the listed General Conditions may result in disqualification of bid.

13.4 In case of tie bids, preference will be given to local bidders.  Consistent and continued tie bidding on any commodity could be cause for rejection of bids by Lubbock Power & Light and/or investigation by the Attorney General to determine possible Anti-Trust violations.

13.5 Before LP&L may award a bid to a nonresident bidder, the nonresident bidder's bid must be lower than lowest bid submitted by a responsible Texas bidder by the same margin or amount that a Texas bidder would be required to underbid the nonresident bidder in the nonresident bidders' home state.

13.6 Any contract made, or purchase order issued, as a result of this Invitation to Bid, shall be entered into the State of Texas and under the laws of the State of Texas.  In connection with the performance of work, the Bidder agrees to comply with the Fair Labor Standard Act, Equal Opportunity Employment Act, and all other applicable Federal, State, and Local laws, regulations, and executive orders to the extent that the same may be applicable.

13.7 Responsible Bidder Criteria:  Lubbock Power & Light shall consider only responsible Bidders.  Responsible Bidders are those that have, in the sole judgment of Lubbock Power & Light, the financial ability, experience, resources, skills, capability, reliability and business integrity necessary to perform the requirements of the contract.  Lubbock Power & Light may also consider references and financial stability in determining a responsible Bidder.

14
EQUAL EMPLOYMENT OPPORTUNITY
14.1 Bidder agrees that it will not discriminate in hiring, promotion, treatment, or other terms and conditions of employment based on race, sex, national origin, age, disability, or in any way violative of Title VII of 1964 Civil Rights Act and amendments, except as permitted by said laws.
15
SPECIFICATIONS
15.1
Any catalog, brand name or manufacturer's reference in the specifications is descriptive and NOT restrictive, and are used to indicate type and quality level desired.  Bids on brands of like nature and quality may be considered unless specifically excluded.

15.2
If bidding on other than reference or specifications, bid must show manufacturer, brand, trade name, catalog and/or lot number, etc., on article offered and certify article offered is equivalent to specifications.  If other than specified brand of items are offered, specifications, catalog sheets, illustrations and complete descriptive literature must be submitted with bid.  

15.3
Minor deviations from written specifications shall not necessarily disqualify a vendor's bid.  Lubbock Power & Light specification committee will be the sole determiner of what constitutes a minor deviation.

15.4
Lubbock Power & Light may deem it necessary to specify Approved Brands after conclusive testing, prior to usage or standardization.  Lubbock Power & Light may test any sample(s), supplied free of charge, to qualify for the Approved Brand list.  Each sample must be marked with bidder's name and address.  At bidder's request and expense, the sample(s) not destroyed or used in examinations and testing will be returned.  

15.5 When specifications call for samples to be submitted, samples shall be delivered by the bidder, at bidder's expense, five days prior to the opening of bids.  Each sample shall be clearly tagged to show bidder's name and address and item number.

15.6 Lubbock Power & Light reserves the right to determine which specific items on any specification requirements require strict adherence, or are most important, and those that are not, or requiring a lesser degree of importance (i.e., the shade of paint is far less important than the horsepower of a motor). Such determination can and will be a basis for evaluating, recommending and making award. Lubbock Power & Light will, at its sole discretion, assess warranty offered, and utilize life-cycle costing and/or performance factors as the evaluation method and basis for award.  The low bid most closely meeting specifications is usually the bid given the award, although delivery time is sometimes a necessary factor (i.e., a low bid that best meets specifications will not do us much good if delivery is two years from now). Should a requested specification sheet not be submitted with a bid, this is considered non-responsive and therefore may not be considered. PLEASE READ AND RESPOND TO SPECIFICATION REQUIREMENTS CAREFULLY.
16 CONSIDERATION OF LOCATION OF BIDDER’S PRINCIPAL PLACE OF BUSINESS

16.1 Pursuant to Texas Local Government Code 271.9051(b), in purchasing real property or personal property that is not affixed to real property, if LP&L receives one or more bids from a bidder whose principal place of business is in the City of Lubbock and whose bid is within five percent (5%) of the lowest bid price received by LP&L from a bidder who is not a resident of the City of Lubbock, LP&L may enter into a contract with:

(1) the lowest bidder; or

(2) the bidder whose principal place of business is in the City of Lubbock if the Electric Utility Board determines, in writing, that the local bidder offers LP&L the best combination of contract price and additional economic development opportunities for the City of Lubbock created by the contract award, including the employment of residents of the City of Lubbock and increased tax revenues to the City of Lubbock.

16.2 In order to receive consideration, bidders must submit an Affidavit of Eligibility. 

17
QUALIFICATIONS OF BIDDERS
17.1
The Bidder may be required before the award of any contract to show to the complete satisfaction of Lubbock Power & Light that the Bidder or his Subcontractor has the necessary facilities, ability, and financial resources to provide the service specified therein in a satisfactory manner.  The Bidder may also be required to give a past history and references in order to satisfy Lubbock Power & Light in regard to the Bidder's or his Subcontractor's qualifications.  

17.2
Lubbock Power & Light may make reasonable investigations deemed necessary and proper to determine the ability of the Bidder or his Subcontractor to perform the work, and the Bidder shall furnish to Lubbock Power & Light all information for this purpose that may be requested.  Lubbock Power & Light reserves the right to reject any bid if the evidence submitted by, or investigation of, the Bidder fails to satisfy Lubbock Power & Light that the Bidder or his Subcontractor is properly qualified to carry out the obligations of the contract and to complete the work described therein.  Evaluation of the Bidder's or his Subcontractor's qualifications shall include:

a)
The ability, capacity, skill, and financial resources to perform the work or provide the service required;

b)
The ability of the Bidder or his Subcontractor to perform the work or provide the service promptly or within the time specified, without delay or interference;

c)
The character, integrity, reputation, judgment, experience, and efficiency of the Bidder or his Subcontractor;

d)
The quality of performance of previous contracts or services.

18
ANTI-LOBBYING PROVISION
18.1
DURING THE PERIOD BETWEEN BID CLOSE DATE AND THE CONTRACT AWARD, BIDDERS, INCLUDING THEIR AGENTS AND REPRESENTATIVES, SHALL NOT DIRECTLY DISCUSS OR PROMOTE THEIR BID WITH LP&L STAFF EXCEPT IN THE COURSE OF LP&L-SPONSORED INQUIRIES, BRIEFINGS, INTERVIEWS, OR PRESENTATIONS, UNLESS REQUESTED BY LUBBOCK POWER AND LIGHT.  

18.2 This policy is intended to create a level playing field for all potential bidders, assure that contract decisions are made in public, and to protect the integrity of the bid process.  Violation of this provision may result in rejection of the bidder's bid.

19 UTILIZATION OF LOCAL BUSINESS RESOURCES

19.1 Lubbock Power & Light desires, as much as practicable, to stimulate growth in all sectors of the local business community.  Bidders are strongly encouraged to explore and implement methods for the utilization of local resources.

20 PROTEST

20.1 All protests regarding the bid solicitation process must be submitted in writing to the Lubbock Power & Light Purchasing Manager within five (5) business days following the opening of bids. This includes all protests relating to advertising of bid notices, deadlines, bid opening, as well as any protest relating to alleged improprieties with the bidding process.

20.2 FAILURE TO PROTEST WITHIN THE TIME ALLOTTED SHALL CONSTITUTE A WAIVER OF ANY PROTEST.
Lubbock Power & Light is aware of the time and effort you expend in preparing and submitting bids to Lubbock Power & Light. Please let us know of any bid requirement causing you difficulty in responding to our Invitation to Bid. We want to facilitate your participation so that all responsible vendors can compete for Lubbock Power & Light’s business. Awards should be made approximately two to six weeks after the opening date.  If you have any questions, please contact the Lubbock Power & Light Purchasing Manager (806) 775-2170.

II. GENERAL CONDITIONS

**** PLEASE READ CAREFULLY ****
These General Conditions apply to all bids and become a part of the terms and conditions of any bid submitted.  LP&L shall mean Lubbock Power & Light.

1 Quantities:  The quantities appearing in this Invitation to Bid are approximate only and LP&L reserves the right to increase, decrease or delete any or all items.  If the quantities of materials to be furnished are increased, such increase shall be paid for according to the unit prices established for the item.  In making its bid hereunder, the Seller expressly recognizes the rights of LP&L provided herein, and further recognizes that the Seller shall have no claims against LP&L for anticipated profits for the quantities called for, diminished or deleted.

2 Product Guarantee: Seller guarantees equipment or product offered will meet or exceed specifications identified in this bid invitation.  The Seller shall, upon request, replace any equipment or product proved to be defective and make any and all adjustments necessary without any expense to LP&L.  If at any time, the equipment or product cannot satisfactorily meet the requirements of the specifications, the Seller shall upon written request from LP&L, promptly remove such equipment or product without any further expense to LP&L. At LP&L’s request, Seller will provide evidence sufficient to demonstrate such equipment or product meets the foregoing.

3 Invoices:  Seller shall submit separate invoices, in duplicate, on each purchase order or purchase release after each delivery.  Invoices shall indicate the purchase order or purchase release number and the supply agreement number if applicable.  Invoices shall be itemized and transportation charges, if any, shall be listed separately.  A copy of the bill of lading, and the freight waybill when applicable, shall be attached to the invoice.  Mail to Accounts Payable, Lubbock Power & Light, P.O. Box 2000, Lubbock, Texas 79457.  Payment shall not be due unless and until the Seller shall not be in default under the terms of the contract, and until the above instruments are submitted after delivery. LP&L MAY MAKE PAYMENTS FOR PURCHASES UNDER THIS CONTRACT USING City of Lubbock’s MASTERCARD PURCHASING CARD (PCARD). THE SELLER AGREES TO ACCEPT PCARD PAYMENTS WITHOUT ANY ADDITIONS OR SURCHARGES.

4 Delivery Delay: When delivery delay can be foreseen, the Seller shall give prior notice to the Purchasing Manager, who shall have the right to extend the delivery date if reasons for delay appear acceptable.  The Seller must keep the Purchasing Manager informed at all times of the status of the order.  Default in any manner under the contract, including, but not limited to default on promised delivery, without acceptable reasons, or failure to meet specifications hereunder authorizes the Purchasing Manager to purchase goods elsewhere and charge any increase in cost and handling to the defaulting Seller, and/or exercise any and all rights available to it by law, equity and/or under the terms of the contract.  Every effort will be made by the Purchasing Office to locate the goods at the same or better price as than originally contracted.

5 Packaging:  Seller will package goods in accordance with good commercial practice.  Each shipping container shall be clearly and permanently marked as follows:  (a) Seller's name and address.  (b) Consignee's name, address and purchase order or purchase release number and the supply agreement number if applicable, (c) Container number and total number of containers, e.g., box 1 of 4 boxes, and (d) the number of the container bearing the packing slip.  Seller shall bear cost of packaging unless otherwise provided.  Goods shall be suitably packed to secure lowest transportation costs and to conform with requirements of common carriers and any applicable specifications.  LP&L’s count or weight shall be final and conclusive on shipments not accompanied by packing lists.

6 Delivery Time: Deliveries will be accepted only during receiving hours: 9:00 A.M. - 3:30 P.M., Monday through Friday, except on City holidays, at the designated location.

7 Damage: LP&L assumes no liability for goods delivered in damaged or unacceptable condition.  The Seller must handle all claims with carriers, and in case of damaged goods, shall ship replacement goods immediately upon notification by LP&L.

8 No Warranty By LP&L Against Infringements: As part of the contract for sale, Seller agrees to ascertain whether goods manufactured in accordance with the specifications attached to the contract will give rise to the rightful claim of any third person by way of infringement of the like.  LP&L makes no warranty that the production of goods according to the specification will not give rise to such a claim, and in no event shall LP&L be liable to Seller for indemnification in the event that Seller is sued on the grounds of infringement or the like.  If Seller is of the opinion that an infringement or the like will result, he will notify LP&L to this effect in writing within two weeks after the signing of the contract.  If LP&L does not receive notice and is subsequently held liable for the infringement or the like, Seller will save LP&L harmless.  If Seller in good faith ascertains the production of the goods in accordance with the specifications will result in infringement or the like, the contract shall be null and void.

9 Material Safety Data Sheets: Seller shall provide Material Safety Data Sheets (MSDS) for all chemicals to comply with provisions of the Texas Hazard Communication Act, Title 6, Subchapter D, Chapter 502, Texas Health and Safety Code Ann.  (This Act is corollary to OSHA Standard 29 CRF 1910.1200, which is generally known as the Right to Know Law.)

10 Shipment Under Reservation Prohibited: Seller is not authorized to ship the goods under reservation and no tender of a bill of lading will operate as a tender of goods.

11 Title & Risk Of Loss: The title and risk of loss of the goods shall not pass to LP&L until LP&L actually receives and takes possession of the goods at the point or points of delivery as provided herein.

12 No Replacement of Defective Tender: Every tender of delivery of goods must fully comply with all provisions of the contract as to time of delivery, quality and the like.  If a tender is made which does not fully conform, this shall constitute a breach of the contract and Seller shall not have the right to substitute a conforming tender, provided, where the time for performance has not yet expired, the Seller may reasonably notify LP&L of his intention to cure and may then make a conforming tender within the Contract time but not afterward.

13 Gratuities:  LP&L may, by written notice to the Seller, cancel the contract or purchase order without liability to Seller if it is determined by LP&L that gratuities, in the form of entertainment, gifts or otherwise, were offered or given by the Seller, or any agent or representative of the Seller, to any officer or employee of LP&L with a view toward securing a contract or securing favorable treatment with respect to the awarding or amending, or the making of any determinations with respect to the performing of such a contract.  In the event the Contract is canceled by LP&L pursuant to this provision, LP&L shall be entitled, in addition to any other rights and remedies, to recover or withhold the amount of the cost incurred by Seller in providing such gratuities.

14 Special Tools & Test Equipment: If the price stated on the face hereof includes the cost of any special tooling or special test equipment fabricated or required by Seller for the purpose of filing this order, such special tooling or equipment and any process sheets related thereto shall become the property of LP&L and to the extent feasible shall be identified by the Seller as such.

15 Warranty-Price:  a.  The price to be paid by LP&L shall be that contained in Seller's bid which Seller warrants to be no higher than Seller's current prices on orders by other parties for products of the kind and specification covered by the contract for similar quantities under similar or like conditions and methods of purchase.  In the event Seller breaches this warranty, the prices of the items shall be reduced to the Seller's current prices on orders by other, or in the alternative.  LP&L may cancel the contract without liability to Seller for breach or Seller's actual expenses.  b.  The Seller warrants that no person or selling agency has been employed or retained to solicit or secure the contract upon an agreement or understanding for commission, percentage brokerage, or contingent fee excepting bona fide employees of bona fide established commercial or selling agencies maintained by the Seller for the purpose of securing business.  For breach or violation of this warranty LP&L shall have the right in addition to any other right or rights to cancel the contract without liability and to deduct from the Contract price, or otherwise recover the full amount of such claimed commission, percentage, brokerage, or contingent fee.

16 Safety Warranty: Seller warrants that the product sold to LP&L shall conform to the standards promulgated by the U. S. Department of Labor under the Occupational Safety and Health Act of 1970 and/or any other governmental agency standards or regulations.  In the event the product does not conform to each OSHA or other standards, Seller shall be in default hereunder, and LP&L may exercise and of the remedy provided for herein, including but not limited to return of the product for correction or replacement at the Seller's expense.  In the event Seller fails to make the appropriate correction within a reasonable time, correction made by LP&L will be at the Seller's expense

17 Right of Inspection: LP&L shall have the right to inspect the goods at delivery before accepting them.

18 Cancellation:  LP&L shall have the right to cancel for default all or any part of the undelivered portion of this order if Seller breaches any of the terms hereof including warranties of Seller or if the Seller becomes insolvent and/or files bankruptcy or has bankruptcy filed against it.  Such right to cancellation is in addition to and not in lieu of any other remedies which LP&L may have in law, equity or hereunder.

19 Termination: LP&L may terminate the contract or purchase order in whole, or in part.  Termination hereunder shall be effected by the delivery to the Seller of a "Notice of Termination" specifying the extent to which the contract or purchase order is terminated and the date upon which such termination becomes effective.  In the event of said termination, in whole or in part, provided that Seller shall not be in default under the Contract, the Seller shall be entitled to payment only for goods actually delivered, and/or services actually performed under and in compliance with the terms of the contract or purchase order.

20 Force Majeure: Neither party shall be held responsible for losses or damages hereunder, if the fulfillment of any terms of provisions of the contract is delayed or prevented by strike, walkouts, acts of God, or public enemy, fire, or flood.

21 Assignment-Delegation:  No right or interest in the contract shall be assigned or delegation of any obligation made by Seller without the written permission of LP&L   Any attempted assignment or delegation by Seller shall be wholly void and totally ineffective for all purposes unless made in conformity with this paragraph.

22 Waiver:  No claim or right arising out of a breach of the contract can be discharged in whole or in part by a waiver or renunciation of the claim or right unless the waiver or renunciation is supported by consideration and is in writing signed by the aggrieved party.

23 Interpretation-Parole Evidence: This writing, plus any specifications for bids and performance provided by LP&L in its advertisement for bids and any other document provided by Seller as part of his bid, is intended by the parties as a final expression of their agreement and is intended also as a complete and exclusive statement of the terms of their agreement.  Whenever a term defined by the Uniform Commercial Code is used in the contract, the definition contained in the Code is to control.

24 Applicable Law: The Contract shall be governed by the Uniform Commercial Code.  Wherever the term "Uniform Commercial Code" is used, it shall be construed as meaning the Uniform Commercial Code as adopted in the State of Texas as effective and in force on the date of the contract.

25 Right To Assurance: Whenever one party to the contract in good faith has reason to question the other party's intent to perform he may demand that the other party give written assurance of this intent to perform.  In the event that a demand is made and no assurance is given within five (5) days, the demanding party may treat this failure as an anticipatory repudiation of the Contract.

26 Indemnification:  Seller shall indemnify, defend, keep and save harmless LP&L, its agents, officials and employees, against all injuries, deaths, loss, damages, claims, patent claims, suits, liabilities, judgments, costs and expenses, which may in anywise arise or accrue against LP&L in consequence of the granting of the contract or which may anywise result there from, whether or not it shall be alleged or determined that the act was caused through negligence or omission of the Seller or its employees, or of the subcontractor or assignee or its employees, if any, and the Seller shall, at his own expense, appear, defend and pay all charges of attorneys and all costs and other expenses arising there from or incurred in connection therewith, and, if any judgment shall be rendered against LP&L in any such action, the Seller shall, at its own expenses, satisfy discharge the same.  Seller expressly understands and agrees that any bond required by the contract, or otherwise provided by Seller, shall in no way limit the responsibility to indemnify, keep and save harmless and defend LP&L as herein provided.

27 Nonappropriation: All funds for payment by LP&L under this contract are subject to the availability of an annual appropriation for this purpose by LP&L.  In the event of nonappropriation of funds for the goods or services provided under the contract, LP&L will terminate the contract, without termination charge or other liability, on the last day of the then-current fiscal year or when the appropriation made for the then-current year for the goods or services covered by this contract is spent, whichever event occurs first.  If at any time funds are not appropriated for the continuance of this contract, cancellation shall be accepted by the Seller on thirty (30) days prior written notice, but failure to give such notice shall be of no effect and LP&L shall not be obligated under this contract beyond the date of termination.

28 Time:  It is hereby expressly agreed and understood that time is of the essence for the performance of the contract, and failure by Seller to meet the time specifications of the contract will cause Seller to be in default of the contract.

29 Silence of Specification: The apparent silence of specifications as to any detail, or the apparent omission from it of a detailed description concerning any point, shall be regarded as meaning that only the best commercial products and practices are to prevail and that only material and workmanship of the finest quality are to be used. All interpretations of the specifications in this bid shall be made on the basis of this statement. The items furnished under this contract shall be new, unused, of the latest product in production to commercial trade, and shall be of the highest quality as to materials used and workmanship. Manufacturer furnishing these shall be experienced in design and construction of such items and shall be an established supplier of the item bid.

SPECIFICATIONS FOR EQUIPMENT

GENERAL INFORMATION, REQUIREMENTS AND CONDITIONS

SCOPE
The specifications attached are for automobiles, trucks and industrial equipment required by Lubbock Power & Light.  Bids shall meet or exceed the minimum requirements for the equipment described by the specification attached. All inquiries made concerning the specifications shall be made to the Purchasing Manager or his designee. Although it is not a requirement for quotation, vendors are strongly encouraged to attend the scheduled pre-bid meeting covering the equipment specified.

APPLICABLE SPECIFICATIONS, STANDARDS, RULES AND REGULATIONS
Automobiles and trucks shall meet or exceed the minimum requirements of the specification and all applicable requirements of Federal Motor Vehicle Safety Standards (Public Law 89-563).  All requirements of these specifications shall be met unless they are in conflict with the applicable Federal Motor Vehicle Standards.

Equipment furnished for the specification shall meet all applicable requirements of the Environmental Protection Agency’s Exhaust Emission Standards (940 CFR 85) as issued under authority of the Clean Air Act, as amended, (42 USC 1857, et seq,).  It shall be the responsibility to the vendor to ensure that the equipment furnished meets the most recent requirements of all applicable laws.  In the event equipment is furnished that is not in compliance with the law, it shall be the responsibility of the vendor to make all necessary modifications to the equipment required to achieve compliance with these laws.

Automobiles and trucks furnished to this specification shall be provided with lamps, signals and reflectors as specified in the Texas “Uniform Act Regulating Traffic on Highways”, (VTCS 6701d as may be amended, modified, and/or codified).

Vehicles, including station wagons designed or used primarily for the transportation of persons, that have a wheelbase longer than 113 inches or that have more than 145 SAE net horsepower, may not be furnished to this specification (Section 3.29, Article 601b, VTCS as may be amended, modified and/or codified).  This provision does not apply to the purchase or lease of vehicles used primarily for criminal law enforcement, or a bus, motorcycle, pickup, van, truck, three-wheel, tractor, or ambulance.

Reference to specifications, standards, and test methods shall be to those in effect on the date of the Invitation for Bids.  The following publications form a part of this specification to the extent specified herein:

ASTM Standards - American Society for Testing and Materials, 1916 Race Street, Philadelphia, Pennsylvania 19103:

ASTM A 606 - Standard Specification for Steel sheet and Strip, Hot-Rolled and Cold Rolled, High Strength, Low-Alloy, with improved Corrosion Resistance.

ASTM A 607 - Standard Specification for Steel Sheet and Strip, Hot-Rolled and Cold-Rolled, High Strength, Low-Alloy Columbium and Vanadium.

Federal Publications - Superintendent of Documents, U.S. Government Printing Office, Washington D.C. 20402.

FMVSS - Federal Motor Vehicle Safety Standards (Public Law 89-563):


(a)
No. 108 - Lamps, Reflective Devices, and Associated Equipment.

(b)
No. 209 - Seat Belt Assemblies for Passenger Cars, Multipurpose Passenger Vehicles, Trucks, and Buses.

(c)
No. 210 - Seat Belt Assembly Anchorage’s - Passenger Cars, Multipurpose Passenger Vehicles, Trucks, and Buses.


(d)
No. 301-75 - Fuel System Integrity.

Federal Standards:


(a)
No. 595 - Colors

CFR - Code of Federal Regulations, Title 40, Part 85 - Control of Air Pollution from New Motor Vehicles and New Motor Vehicle Engines, Environmental Protection Agency.

DOT - Department of Transportation, Title 49, Part 393 - Liquid fuel Systems of Commercial Motor Vehicles, Certification of Fuel Tank.

OSHA - Occupational Safety and Health Administration - Construction Safety and Health Regulations Section 1926.601 - Motor Vehicles.

SAE - Society of Automotive Engineers, 400 Commonwealth Drive, Warrendale, Pennsylvania 15096:

J377 - SAE Standard - Performance of Vehicle Traffic Horns.

TBEA - Truck Body Equipment Association, 5530 Wisconsin Avenue, Suite 120, Washington D.C. 20015:

VTCS - Vernon’s Texas Civil Statutes - West Publishing Company, P.O. Box 2239, Kansas City, Missouri 64142:

VTCS - 670ld, as may be amended, modified, and/or codified - Uniform Act Regulating Traffic on Highways.

GENERAL INFORMATION AND REQUIREMENTS
The vehicles furnished under this specification shall be either new or current production models and shall be of good quality workmanship and material.  The bidder represents that all units offered under this specification shall meet or exceed the minimum requirements specified for each vehicle series listed.

Successful bidders shall furnish automobiles and trucks equipped exactly as listed for makes and models in this specification and with any other requirements specified in the Invitation for Bids.  The vehicles shall be completely assembled, serviced, adjusted, and all equipment including standard and optional equipment shall be installed and the units made ready for continuous operation.  Standard equipment means those components and accessories usually and ordinarily furnished without additional cost on regular production models.  Each vehicle must be supplied with an owner/operator manual.  Bids are to include unit pricing for one set of manufacturer's repair, parts and service manuals (hard copy and on CD Computer Disk).

No equipment mounted on trucks shall, under any circumstances, be welded to the vehicle at any point between the front of the front spring hanger and the rear of the rear spring hanger.  Also, all holes for bolting must be drilled in the accepted manner and the burning of said holes shall not be acceptable under any condition.  Further, no holes shall be drilled in top or bottom flange of truck frame unless drilling is confined to the section behind the rearmost attachment of the rear spring hangers.  Welding or torch cutting shall be confined to “boxing” the rear end of truck frame (as required for dump equipment to allow full dumping angle).  All such work shall be confined to area behind rear spring hangers.  Mounting strip between hoist subframe of dump body and truck frame may have flame cut holes to countersink rivets on truck frame.  Chassis frame rivets shall not be removed or cut flush with frame for any reason.

Quantities, color, mounting and other requirements for lamps, signals, and reflectors shall be as specified for vehicles by Federal Motor Vehicle Safety Standard No. 108.

Reflectors and clearance, side-marker and identification lamps for vehicles requiring same shall also meet the following requirements.  Reflectors must be housed type with screw or bolt type mounting.  Stick-on type is not acceptable.  Surface-mounted clearance and side-marker lamps must be metal armored type.  Recess mounted side-marker and clearance lamps must be recessed sufficiently to provide protection for the lens.  Lenses for side-marker and clearance lamps shall be secured to the lamp by a fastening method which requires a tool to remove the lens.

All electrical wiring shall be insulated and enclosed in a fibrous loom, plastic loom, or flexible conduit for protection from external damage and short circuits.  It shall be securely fastened at sufficient intervals to prevent sagging and insure clearance of mechanical parts.  Routing of the wiring through the cab, frame, body, compartment box, and the like shall be placed in such a manner so as not to interfere with normal operation and use, or present a safety hazard.

Tires shall be of the type of construction specified under the applicable specification or General Requirements for each series.  All tires shall be new and the tread style furnished shall be the tire manufacturer’s standard design for original equipment line of tires unless otherwise specified in the specifications.  All tires shall be of the quality known as “Original Equipment Line”.  All tires and wheels shall be properly balanced prior to delivery of the unit.

Motorized vehicles shall be delivered with not less than one quarter (1/4) tank of fuel. 

Highway legal vehicles required to display a State of Texas, Department of Public Safety, inspection sticker, shall be furnished with same at time of delivery to the City. Vehicles qualifying for a two-year inspection sticker shall be furnished with the two-year version.

Vehicles equipped with multiple-piece rims will not be accepted.
Calcium hybrid type batteries shall be standard equipment on all equipment furnished as per the attached specification.

Each vehicle, except cab and chassis units, shall be furnished with means and adequate space for attaching the rear license plate, without modifications.  Illumination for the license plate shall be provided to meet Texas Department of Public Safety requirements.  It shall be the responsibility to the vendor who installs the bed or body on the equipment to ensure that this requirement is met as stated above.

Each vehicle shall be equipped with a horn or horns meeting the requirements of SAE J377.

NOTE:
Speedometer drive train must be properly calibrated in relation to axle ratio and tire size to give accurate readings.

CERTIFICATION AND COMPLIANCE
Failure on the part of the bidder to comply with any and all requirements and conditions of this specification may subject his bid to rejection.  No exceptions to or deviations from this specification will be considered unless each exception or deviation is specifically stated as a part of the bid.  Any exception must be specifically stated by the bidder as an exception with a detailed statement completely defining the exception and/or exceptions.  This detailed exception must be listed on the specification in the space provided and on a separate sheet of paper, clearly labeled as an exception, along with the item number of the exception and attached to the bid.  The make and model number must be shown on each bid, however, this information will not be sufficient evidence that the bidder is making an exception.  If no exceptions or deviations are shown, the bidder will be required to furnish vehicles and equipment exactly as specified herein. The burden of proof of compliance with this specification shall be the responsibility of the vendor.
Bidders must submit with their bids, or have on file with Lubbock Power & Light, the latest printed literature on equipment the bidder proposes to furnish.  This literature shall include an engine chart showing net horsepower, net torque, and other characteristics of the equipment quoted.  The specifications for each piece of equipment quoted shall be returned with the quote and shall be clearly marked by each item on the specification.  This document becomes a part of the evaluation process and is required for this purpose.

TRADE-INS
If there is a trade-in, it is offered at LP&L’s option, WHERE IS AND AS IS AND WITH ALL FAULTS, and the Dealer must take possession at the location listed and remove the trade-in from LP&L’s premises within 30 days from delivery date of new equipment, or within such time otherwise dictated by the Contract.

Lubbock Power & Light makes no representation or warranty whatsoever about the condition of the trade-ins listed, either expressed or implied and no agent or employee of LP&L is authorized to make representation or warranty as to the condition of the trade-ins offered.  The purchaser shall have no claim against LP&L for the condition of trade-ins offered as a part to the quote.  Therefore, bidders are urged to inspect the trade-in equipment offered as a part of the quotation.  Failure to do so, however, shall not impair or affect any of the terms of this Contract.

WARRANTY AND SERVICE
The Dealer shall furnish the receiving agency a Manufacturer’s Certificate of Origin (Certificate of Title will not meet this requirement), a manufacturer’s new vehicle warranty and a manufacturer’s new vehicle service contract that will be honored by any of the manufacturer’s authorized contractors.  (The 1,000 mile inspection coupon is not required, unless otherwise specified in the Invitation for Bids).  Manufacturer’s new vehicle warranty as offered to the general public shall be furnished on all vehicles delivered to Lubbock Power & Light.  Manufacturer’s Certificate of Origin shall reflect the GVWR required by:  (a) The particular model specification:  (b) The agency’s written exception; or (c) A greater GVWR required by extra equipment.

The Dealer shall furnish a copy of the manufacturer’s standard warranty on major accessories such as dump, stake, platform and utility bodies, side-pak tool compartments, and toolboxes at the time of delivery.

Delayed warranties are available on vehicles.  Specifying them on the Invitation for Bids will give the vendors advance notification of this requirement.  Delays exceeding six (6) months are not acceptable.

Extended warranties available from manufacturer shall be offered and separately priced with response to solicitation.

IMPORTANT: BIDDER MUST SUBMIT WITH THEIR BID DETAILED WARRANTY INFORMATION FOR THE MANUFACTURER'S WARRANTY AND DETAILED WARRANTY INFORMATION FOR THE MANUFACTURER'S EXTENDED WARRANTY. 

FLEET COLOR CHARTS

When requested, the Bidder shall furnish as a part of their bid, manufacturers standard “fleet” color charts, showing interior and exterior colors available for the equipment quoted.

INSURANCE REQUIREMENTS

The successful bidder shall furnish a certificate of insurance, which includes the coverage, and limits set forth below; identifies the City of Lubbock as additional insured; and provides for at least ten (10) days prior notice to LP&L of cancellation or non-renewal:

Comprehensive Commercial General Liability Insurance, including blanket Contractual Liability Insurance, Premises/Operations, Independent Contractors, and Products/Completed Operations Insurance issued by an insurance company licensed to conduct business in the State of Texas with limits not less than: $1,000,000 for all damages because of bodily injury sustained by each person as the result of each occurrence and $2,000,000 bodily injury aggregate per policy year; and limits of $2,000,000 for all property damage aggregate per policy year or a limit of $1,000,000 Combined Single Limit (CSL). All, if any, deductibles are the sole responsibility of the contractor to pay and/or indemnify. 

ORDER ACKNOWLEDGEMENT

For the purchase of a factory-ordered unit, the dealer's Contract shall incorporate the following conditions, as apply to vehicles purchased for Lubbock Power & Light:

1.
A form shall be submitted to the Lubbock Power & Light Fleet Services Manager that describes the exact vehicle to be ordered, with all options and accessories as requested clearly noted;

2.
Within five (5) working days after receipt of purchase order by Dealer and entry into the manufacturer computer, the dealer shall submit to the Lubbock Power & Light Fleet Services Manager, or his designee, a copy of the factory Order Acknowledgment or other confirmation that a factory order for the vehicle(s) was accepted and scheduled by the manufacturer for production, as specified, with the Factory Order Number generated by the manufacturer computer acknowledgement for each vehicle ordered.

The Lubbock Power & Light purchase order, to which will be attached a copy of the vendor's bid and the full text of these Specifications, will be forwarded to the dealer for units accepted for purchase.

Failure to comply with the above conditions is cause for immediate cancellation of the order, and placing of the order for that Item of the bid with another dealer.  There shall be no liability placed on LP&L in the event of cancellation of an order under such circumstances. The manufacturer's fleet account zone representative will be notified should any dealer fail to comply with conditions of LP&L’s bid, or the Contract provisions.

NEW EQUIPMENT SERVICE QUESTIONNAIRE

1.  
What is the name and address of the nearest authorized service facility to the City of Lubbock?  If your company does not own nearest service facility, please provide letter of assurance of service from said facility.

2.
What is your total parts inventory for the proposed equipment?

3.
How many technicians are employed at the nearest service facility?

4.
How many field service technicians are available for on-site service?

5.
What is the hourly labor rate for shop labor?

6.
What is the hourly labor rate for field service labor?

7.
What is the average response time that can be expected for a service call?

8.
What is the average delivery time for parts not found in inventory?

9.
Approximately how long will replacement parts be available for the proposed unit?

10.
Explain the method for calculating the discount available for repair/replacement parts.  (Show percent of discount to be expected.)

11.
Provide an explanation of the standard warranty coverage of the machine quoted.  What is the process for handling defective parts, quality of workmanship or poor quality of materials?

12.
How many years has this particular machine been in production?

13.
If the service facility is located outside the City of Lubbock, explain the process for performing (i) warranty work, (ii) service not covered in the warranty, and (iii) service work after the warranty has expired.

14.
Who is liable for transportation expense should the unit require out of town service during the warranty period?

15.
Explain the method used to calculate the transportation expense of out of town service.

16.
State in years the useful life and expected downtime of equipment quoted.

NOTE:  RETURN THIS QUESTIONNAIRE ALONG WITH YOUR BID SUBMITTAL.  YOUR RESPONSE TO THE EQUIPMENT SERVICE QUESTIONNAIRE MAY BE A FACTOR IN DETERMINING THE LOWEST RESPONSIBLE BID.
LUBBOCK POWER & LIGHT
STATEMENT OF NO BID
Lubbock Power & Light is very conscious and extremely appreciative of the time and effort you expend in preparing and submitting bids to LP&L. If you do not intend to bid on this requirement, please complete and return this form prior to date shown for receipt of bid to: Ron Shuffield, Purchasing Manager Electric Utilities, Lubbock Power & Light, 402 Municipal Drive, Lubbock, Texas 79403. 

We, the undersigned, have declined to bid on your ITB #

 for the following reason(s):


Specifications too “tight”, i.e. geared toward one brand or manufacturer only. (Please explain reason below)

 Specifications unclear. (Please explain below)

 Insufficient time to respond to Invitation to Bid.

_____ We do not offer this product/s or equivalent. (If you wish to remain on bidders list for other commodities and/or services, please state particular product and/or service under which you wish to be classified.)




_____ Our product schedule would not permit us to perform.




_____ Unable to meet specifications.

_____ Job too large.






_____ Job too small.






_____ Cannot provide required bonding.




_____ Cannot provide required insurance.




_____ Bidding through dealer.





_____ Do not wish to do business with the City of Lubbock. (Please explain below)




 Other (Please specify below)
REMARKS:





































































Company Name:











Address:












City:






 State:

 Zip





Contact Name:





 Title:







Business Telephone Number




  FAX:





Internet Address:












Company's Internet Web Page URL:










Lubbock Power & Light

Consideration of Location of Bidder's Principal Place of Business

Affidavit of Eligibility

Pursuant to Texas Local Government Code 271.9051(b), in purchasing real property or personal property that is not affixed to real property, if LP&L receives one or more bids from a bidder whose principal place of business is in the City of Lubbock and whose bid is within five percent (5%) of the lowest bid price received by LP&L from a bidder who is not a resident of the City of Lubbock, LP&L may enter into a contract with:

 (1)
the lowest bidder; or

(2)
the bidder whose principal place of business is in the City of Lubbock if the Electric Utility Board determines, in writing, that the local bidder offers LP&L the best combination of contract price and additional economic development opportunities for the City of Lubbock created by the contract award, including the employment of residents of the City of Lubbock and increased tax revenues to the City of Lubbock.

In order to receive consideration, bidders must submit this affidavit to:

Ron Shuffield, Purchasing Manager Electric Utilities

Lubbock Power & Light

402 Municipal Drive

Lubbock, TX 79403

Complete all areas below. Incomplete affidavits may be rejected.

Local Business Name: 











Local Address (must be within the City limits): 








1. Is the above address the principal place of business for the business named above? 




2. How many residents of the City of Lubbock are employed at the above business location?



3. Year your business was established in the City of Lubbock: 






4. For transactions that require sales tax, provide the following Reseller information:

Reseller Permit Number: 










Company Name and Address (as it appears on permit):

5. Does your business have more than one office in the State of Texas? 

 Yes  

 No

If Yes, identify the office location considered as the point-of sale for the purpose of sales tax calculation:

6. Was the local business required to pay business and/or real property tax for the most recent tax year? 


 Yes
 
 No  

If Yes, did the local business pay any of this tax to the City of Lubbock?

 Yes

 No

Under penalty of perjury, the undersigned states that the foregoing statements are true and correct.  It is further acknowledged that any person, firm, corporation or entity intentionally submitting false information to the City in an attempt to qualify for eligibility shall be prohibited from bidding on City of Lubbock products and services for a period of one (1) year.

Authorized Signature: 






 Date: 




Printed Name and Title: 












LUBBOCK POWER & LIGHT

MINIMUM SPECIFICATIONS

FOR

6 YARD DUMP BODY WITH HYDRAULIC HOIST 

SPEC # 7313-100

MAKE 


 MODEL 



IT IS THE INTENT OF THIS SPECIFICATION, REFERENCED DOCUMENTS, REQUIREMENTS AND CONDITIONS SECTIONS TO DESCRIBE MINIMUM PERFORMANCE REQUIREMENTS.  THE VEHICLE OR PRODUCT SHALL MEET OR EXCEED THE PERFORMANCE OR CONSTRUCTION DESCRIBED HEREIN. THE VENDOR SHALL BE REQUIRED TO MARK COMPLIANCE OR NON-COMPLIANCE TO EACH ITEM DESCRIPTION IN THE SPACE PROVIDED. SPECIFICATION ITEMS LEFT BLANK WILL AUTOMATICALLY BE INTERPRETED AS A “NO” FOR THAT PARTICULAR ITEM (S).   ALL EQUIPMENT FURNISHED AS STANDARD TO THE GENERAL PUBLIC ON THE PRODUCT BY THE MANUFACTURER SHALL BE INCLUDED, EVEN WHEN NOT SPECIFICALLY IDENTIFIED IN THIS SPECIFICATION. ANY DEVIATIONS FROM THE WRITTEN SPECIFICATION WITH DATE AS SHOWN IN THE INVITATION TO BID (ITB) SHALL BE NOTED ON THE ATTACHED EXCEPTIONS TO THE SPECIFICATION. IN ORDER TO RECEIVE FULL CONSIDERATION, ITB RESPONSE QUOTATION MUST FOLLOW THIS SPECIFICATION AND THE INVITATION TO BID'S TERMS AND CONDITIONS.

NO.
ITEM
MINIMUM REQUIREMENTS
SELLER COMPLIANCE


YES
NO


	
	EXCEPTIONS   

	vendor EXCEPTIONS or additions shall be listed on the sheet provided at end of this bid. do list items on the  bid
	
	
	

	
	Dump body
	THIS SPECIFICATION DESCRIBES A DUMP BODY, OF 6 CUBIC YARD HEAPED CAPACITY, 5  YARD WATER LEVEL WITH HINGED TAIL GATE, AND HYDRAULIC HOISTING ASSEMBLY FURNISHED AND INSTALLED UPON A Two AXLE CHASSIS WITH 33,000 LBS 
	
	
	

	1.
	DUMP BODY
	GALION 400U/T BODY WITH A 5384 CU YD OR LP&L APPROVED EQUAL 
	
	
	

	2.
	DIMENSIONS
	120” INSIDE LENGTH, 84” INSIDE WIDTH
	
	
	

	3.
	HEAD/TAIL BOARD
	FRONT: 36” ABOVE BODY FLOOR HEIGHTS.


TAIL: 36” ABOVE BODY FLOOR HEIGHTS
	
	
	

	4.
	TAILGATE
	ONE PIECE, SIX PANELTAILGATE, INCLUDING TWO INTERMEDIATE

VERTICAL BRACES AND ONE INTERMEDIATE HORIZONTAL BRACE.
DOUBLE ACTING DESIGN WITH LONG CHAINS AND TWO SETS OF

BANGO EYES AND FULL WIDTH LOWER TAILGATE PIN.
	
	
	

	5.
	HEIGHT ON SIDES
	30”, 8 GA. METAL SIDES WITH 6” STEEL SIDEBOARD EXTENSIONS
	
	
	

	6.
	BODY CAPACITY
	6 CUBIC YARDS HEAPED CAPACITY.
	
	
	

	7.
	PTO
	HOT SHIFT PTO, AIR OPERATED PTO ENGAGEMENT WITH CONTROLS MOUNTED CONVENIENT TO OPERATOR’S REACH.
	
	
	

	8
	HOIST
	GALION # 6384NTEA  APPROVED CLASS 50, 17.7 TON CAPACITY.
	
	
	

	9.
	CYLINDER
	SHALL BE A 84” STROKE OF MULTI-STAGE DESIGN, WITH HOLDING 

FEATURE PREVENTING BED FALLING IN THE EVENT OF LINE

FAILURE.
	
	
	

	10.
	HYDRAULIC PUMP
	MOUNTED DIRECT-COUPLED HIGH-PRESSURE

GEAR TYPE PUMP, FURNISHED WITH CAB MOUNTED AIR

OPERATED PTO ENGAGEMENT
	
	
	

	11.
	HYDRAULIC RESERVOIR
	RESERVOIR SHALL BE GALION STANDARD CAPACITY.  MOUNTED RESERVIOR SHALL BE EQUIPPED WITH A SHUT OFF VALVE CAPABLE OF SHUTTING OFF ALL FLOW FROM TANK.
	
	
	

	12.
	METAL GAUGES   
	CONSTRUCTION ON SIDES AND FLOOR SHALL BE WEAR RESISTANT 8 GAUGE HIGH TENSILE STEEL WITH A TWO (2”) FLOOR TO SIDE RADIUS.
	
	
	

	13.
	MAIN FRAME
	LONGITUDINAL RAILS SHALL BE TWO (2), 6” STRUCTURAL CHANNEL
	
	
	

	14.
	CROSS MEMBERS
	MINIMUM 4” STRUCTURAL CHANNEL ON 12” CENTERS GUSSETED 

TO MAIN FRAME RAILS
	
	
	

	15.
	TAILGATE BRACES
	SLOPING TOP SURFACE AT EACH SIDE TO CONNECT TO 

SIDEBOADS
	
	
	

	16.
	CAB PROTECTION
	CAB PROTECTION MINIMUM ¾ CAB, FULL WIDTH, CAB PROTECTION.
	
	
	

	17.
	UNDERCOATING
	DUMP BODY SHALL BE UNDERCOATED TO PREVENT RUST
	
	
	

	18.
	PAINT FINISH
	BODY AND ATTACHMENTS SHALL BE CLEANDED PRIMED AND PAINTED WITH ACRYLIC ENAMEL OR POLY TYPE PAINT FINISH COLOR BLACK
	
	
	

	19.
	BUCK PLATE   
	THE REAR OF TRUCK SHALL BE PROVIDED WITH A HEAVY DUTY BUCK PLATE WITH THE FOLLOWING: TWO SAFETY RINGS, A SAE/ICC SIX (6) WAY FEMALE TRAILER PLUG, WIRED TO DOT GUIDELINES.  IF CAB CHASSIS CAME EQUIPPED WITH A 7 WAY PLUG IT TOO SHALL BE MOUNTED IN THE BUCK PLATE.  
	
	
	

	20.
	PINTLE  HITCH
	A HOLLAND PH-775SL  PINTLE HITCH MOUNTED TO THE BUCKBOARD AT THE HEIGHT OF  AT 24 (+/-2”) INCHES AND BE BRACED TO FRAME OF THE TRUCK. 
	
	
	

	21.
	LADDER
	THE DUMP BODY SHALL HAVE  A LADDER ON THE DRIVERS SIDE WITH ONE STEP INSIDE  BED FOR EASY ENTRY INTO BED  
	
	
	

	22.
	LIGHTS
	STOP/TAIL/TURN LIGHTS SHALL BE 4 INCH TRUCKILTE SUPER 44 LED IN A FLUSH SHOCK ABSORBING RUBBER.  ALL MARKER LIGHTS  SHALL ALSO BE LED TYPE. 
	
	
	

	23.
	TOOLBOXES
	TWO, water tight weatherguard TOOLBoxes 30” length, 18” depth, 18” heighT. both TO BE A DROP DOOR Toolbox.  BOLT TO ¼” X 2” ANGLE mounted TO FRAME OF TRUCK. brackets shall not be welded to frame or body

weatherguard Model 530-3-01
	
	
	

	24.
	TRAILER BRAKE CONTROLLER


	TRAILER BRAKE CONTROLLER SHALL BE A KELSEY-HAYES

AIR OVER ELECTRIC AND WIRED TO A SIX WAY BERG PLUG

ON TAIL BOARD OF TRUCK. 
	
	
	

	25.
	Wiring                                      
	Where wires are run through metal, rubber grommets

shall be used to protect wires from chaffing.  WIRES

SHALL BE DOT COLOR CODED.
	
	
	


	26.
	REPAIRS
	BIDDER SHALL START REPAIRS  WITHIN TWELVE HOURS (12) OF

NOTICE BY LUBBOCK POWER & LIGHT. TRAVEL EXPENSES AND

TRANSPORT OF THE VEHICLE FOR REPAIRS SHALL BE THE

RESPONSIBILITY OF THE BIDDER IF UNIT IS UNDER WARRANTY.
	
	
	

	27.
	DEALER / SERVICE  CENTER                                  
	THE BIDDER SHALL BE A FACTORY AUTHORIZED service center, WITH COMPLETE PARTS AND SERVICE for THE DUMP

BODY, COMPONENTS OF THE HYDRAULIC SYSTEM  AND CONTROLS.  BIDDER SHALL SUBMIT WITH THE BID CURRENT PRINTED LITERATURE AND SPECIFICATION  SHEETS ON THE UNIT OFFERED IN RESPONSE TO SOLICITATION. A COPY OF  FACTORY AUTHORIZED SERVICE CENTER SHALL ALSO BE attached to bid.  If not an AUTHORIZED SERVICE CENTER LIST NEAREST MILEAGE AND NAME OF DEALER.
	
	
	

	28.
	SERVICE CENTER
	If not an AUTHORIZED SERVICE CENTER, LIST one in SPACE PROVIDED BELOW.

DEALER  NAME    ______________________________  

City                        __________________________________
MILEAGE              ______________________________ 

	
	
	

	29.
	WARRANTY
	THE INSTALLATION SHALL BE 100% WARRANTED,

 PARTS AND LABOR, FOR NOT LESS THAN  0ne (1) YEAR AFTER

ACCEPTANCE AND PLACED IN SERVICE BY LUBBOCK POWER &

 LIGHT.                                                                                                             
	
	
	

	30.
	MSO / TITLE
	MSO / TITLE application SHALL BE MADE OUT TO THE CITY OF

LUBBOCK. A CERTIFIED WEIGHT SLIP SHALL BE DELIVERED WITH the UNIT.  Vendor  shall ALSO certify the vehicle as a completed unit TO BE  DELIVERED TO 402 MUNICIPAL DR.
	
	
	


	
	TRUCK CHASSIS  SPEC
	
	
	
	

	1.
	 CHASSIS  
	 A TWO AXLE CHASSIS, 6X4 WITH A CONVENTIONAL CAB. 
	
	
	

	2.
	WHEEL BASE
	cab CHASSIS AXLE MEASURMENT WILL be DETERMINED BY VENDOR TO BE CORRECT LENGTH FOR BED BID.
	
	
	

	3.
	GVWR
	 thirty-three THOUSAND (33,000) POUNDS GROSS VEHICLE 

 WEIGHT RATING.
	
	
	

	4.
	FRONT AXLE
	SET BACK, 12,000 POUNDS MINIMUM, WITH OIL TYPE HUBCAPS  WITH VIEW WINDOW
	
	
	

	5.
	REAR AXLE
	twenty-one THOUSAND ( 21,000) POUNDS multi-leaf, 

WITH DUAL TIRES. TRUCK SHALL ALSO HAVE 4500LB OEM Auxiliary OVERLOAD Springs.
	
	
	

	6.
	AXLE RATIO
	Rear axle ratio should just provide max start and 2.5% at 65 mph fully loaded.
	
	
	

	7.
	SHOCKS
	MANUFACTURER’S FRONT AXLE, HEAVY DUTY SHOCKS.
	
	
	

	8.
	SPRINGS
	OEM SUSPENSION RATED FOR GVWR. 
	
	
	

	9.
	ENGINE
	HIGH TORQUE DIESEL, RATED AT 300 HORSE POWER WITH NOT LESS THAN  800 FT. LBS. TORQUE 
	
	
	

	10.
	EXHAUST
	SINGLE HORIZONTAL MUFFLER WITH HORIZONTAL TAIL PIPE SHALL BE  RIGHT-HAND MOUNTED 
	
	
	

	11.
	BLOCK- HEATER                       
	PHILLIPS-TEMRO 1000 WATT/115 VOLT BLOCK HEATER CHROME ENGINE HEATER RECEPTACLE MOUNTED UNDER LEFT HAND DOOR. sHALL HAVE A CORD TO PLUG INTO 120 VOLTS  
	
	
	

	12.
	TRANSMISSION
	TRANSMISSION SHALL BE A 6 SPEED ALLISON MODEL3500 RDS. CONTROLS SHALL BE DASH MOUNTED 
	
	
	

	13.
	TIRES 
	11R X 22.5 RADIALS. FRONT TIRES WITH HIGHWAY TREAD WITH MUD AND SNOW TREAD ON THE DRIVE AXLES. ALL TIRES SHALL BE GOODYEAR TO LOWER REPLACMENT COST.
	
	
	

	14.
	WHEELS
	10-HOLE DISK TYPE, 22.5 X 8.25, TUBELESS
	
	
	

	15.
	BRAKES
	FULL AIR BRAKE SYSTEM CONFORMING TO DOT REQUIREMENTS WITH OUTBOARD MOUNTED REAR BRAKE DRUMS.
	
	
	

	16.
	AIR DRYER
	THE AIR BRAKE SYSTEM SHALL BE FURNISHED WITH AUTOMATIC DRAIN VALVE ON THE WET TANK AND A HEATED AIR DRYER


	
	
	


	17.
	STEERING
	MANUFACTURER'S STANDARD POWER ASSISTED
	
	
	

	18.
	FUEL TANKS
	OEM DUAL STEP TANKS WITH NOT LESS THAN 80 GAL CAPACITY. 
	
	
	

	19.
	FRAME / BUMPER                   
	OEM double frame rated for sever duty SHALL BE CLEAR FROM BACK OF CAB TO REAR OF TRUCK. BRACKETS AND SPRING HANGERS SHALL BE BOLTED. 

       
	
	
	

	20.
	INSTRUMENTS
	OEM FULL GAUGE INSTRUMENT DISPLAY TO INCLUDE ENGINE 

OIL PRESSURE, COOLANT TEMPERATURE, BATTERY CHARGE

INDICATOR, TACHOMETER AND ENGINE HOUR METER
	
	
	

	21.
	THROTTLE
	VERNIER LOCKING TYPE OR ELECTRICAL CONTROLLED HIGH

IDLE SPEED
	
	
	

	22.
	ALTERNATOR
	OEM HEAVY TRUCK TYPE ALTERNATOR, WITH NOT LESS THAN 

160 AMP RATING.
	
	
	

	23.
	BATTERY
	DUAL 700 CCA FRAME MOUNTED WITH EXTERNAL POST FOR JUMP STARTING
	
	
	

	24.
	SEATS
	INTERIOR COLOR, DARK CHARCOAL IN COLOR TO INCLUDE A OEM FULL CLOTH FABRIC COVER WITH HIGH BACKS.  UNIT SHALL HAVE MAXIUM SOUND DEADENING INSULATION THAT INCLUDES A HEADLINER
	
	
	

	25.
	A/C, HEATER 
	OEM STANDARD AIR CONDITIONER heating WITH DASH OUTLETS 
	
	
	

	26.
	MIRRORS
	HEATED, WEST COAST TYPE, WITH A SEPARATELY MOUNTED convex type one on each side

  
	
	
	

	27.
	GLAZING
	OEM  WINDOWS WITH deep TINTED GLASS.  
	
	
	

	28.
	GRAB HANDLES
	OEM GRAB HANDLES  MOUNTED ON each side of  the CAB L&R

BEHIND DOORS
	
	
	

	29.
	12V-DC OUTLET
	TWO OEM STANDARD POWER OUTLETS INSIDE CAB .
	
	
	

	30.
	RADIO
	OEM AM/FM WITH TWO SPEAKERS AND CLOCK DISPLAY.
	
	
	

	31.
	WIPERS
	OEM 2 SPEED WITH INTERMITTENT FEATURE AND WASHERS
	
	
	

	32.
	HORNS
	OEM ELECTRIC AND AIR HORNS. AIR HORNS TO BE MOUNTED 

UNDER HOOD
	
	
	

	33.
	Bumper
	FRONT BUMPER SHALL BE  ¼  THICK WITH SWEPT BACK ENDS. 
	
	
	

	34.
	BACKUP ALARM
	AN AUTOMATIC ACTING, ELECTRIC BACKUP ALARM.
	
	
	

	35.
	TOW HOOKS
	TWO (2) EACH, TOW HOOKS OEM MOUNTED ON FRONT OF THE FRAME



	
	
	

	36.
	WIRING
	OEM WIRING SHALL BE ROUTED TO THE END OF THE FRAME FOR UPPFITERS USE.
	
	
	

	37.
	 PAINT COLOR
	TRUCK SHALL BE OEM fleet WHITE COLOR WITH A BLACK FRAME. THE BED SHALL BE PREPAIRED, PRIMED AND PAINTED WITH BLACK

URETHANE PAINT. 


	
	
	

	38.
	 demonstration
	VENDOR MAY BE REQUIRED TO DO AN ONSITE demonstration OF UNIT AT NO COST TO LP&L FOR BID FOR ACCEPTANCE.
	
	
	

	
	
	
	
	
	

	39.
	manufacturer’s print-out 
	Bidder shall provide a manufacturer’s print-out (Ford “DORA”/“Commerical Truck Tools”, Freightliner “Spec Pro”,   International “Vehicle Specifications”, Mack “Order/Customer/Vehicle Information”, or approved equivalent to verify the vehicle bid meets all the requirements of this specification. Also, any dealer installed aftermarket components, if specified, must be noted  
	
	
	

	40.
	warranty  Delay
	all warrantIES shall have a Delay in warranty start date to allow for body installation. Warranty to become effective when vehicle is placed IN SERVICE BY LUBBOCK POWER & lIGHT in service rather than at time of delivery.
	
	
	

	41.
	DUMP BED WARRANY
	THE DUMP BODY AND COMPONENTS OF THE HYDRAULIC SYSTEM CONTROLS AND THE INSTALLATION SHALL BE 100% WARRANTED PARTS AND LABOR FOR NOT LESS THAN 0NE (1) YEAR AFTER ACCEPTANCE BY LP&L.
	
	
	

	42.
	LITERATURE
	ALL manufacturer’s LITERATURE FOR BED, CAB CHASSIS AND EQUIPMENT SHALL BE ATTACHED TO THE BID 
	
	
	

	43.
	modificationS
	Welding shall not BE permitted on the frame side rails, nor shall the frame rails be cut to lengthen or shorten the wheelbase. Wheelbase modifications are allowed only by sliding the suspension with the “AF” dimension affected accordingly (excess length behind the rear axle may be cut off as required). Any wheelbase modification shall result in a wheelbase and frame combination that is identical to one available from the manufacturer. 
	
	
	


	 44.
	AUTHORIZED WARRANTY CENTER


	THE BIDDER SHALL BE  A FACTORY AUTHORIZED, WARRANTY CENTER WITH COMPLETE PARTS,  SERVICE OF  CAB CHASSIS, DUMP BODY, COMPONENTS OF THE HYDRAULIC SYSTEM  AND CONTROLS. 

BIDDER SHALL SUBMIT  PROOF  OF FACTORY AUTHORIZED SERVICE CENTER. SHALL BE attached to bid ALONG WITH SPECIFICATION  SHEETS OFFERED IN RESPONSE TO SOLICITATION.   
	
	
	

	45.
	SERVICE CENTER
	If not an AUTHORIZED SERVICE CENTER, LIST one in SPACE PROVIDED BELOW.

DEALER  NAME    ______________________________  

City                        __________________________________
MILEAGE              ______________________________ 

	
	
	

	46.
	MSO /  TITLE application
	 MSO / TITLE application SHALL BE MADE OUT TO THE CITY OF LUBBOCK. AND A CERTIFIED WEIGHT SLIP SHALL BE DELIVERED WITH the UNIT. Vendor shall ALSO certify the vehicle as a  completed unit.  DELIVER compeleted unit TO 402 MUNICIPAL DR. unit shall be delivered with a certified weight slip and four (4) set of keys.

	
	
	

	
	
	OPTIONS

	
	
	

	1.
	CAB CHASSIS EXTENDED WARRANTY
	OEM manufacturer’s OEM EXTENDED WARRANTY SHALL INCLUDE THE COMPLETE CHASSIS, ENGINE AND OEM ATTACHED COMPONENTS, RADIATOR, FAN CLUTCH, IDLER PULLEYS, TRANSMISSION, AND SELECTOR CONTROLS, DRIVELINES AND U-JOINTS, ELECTRICAL SYSTEM INCLUDING OEM WIRE HARNESS, ALTERNATOR, STARTER, DASH INSTRUMENTATION AND CONTROLS, FULL SUSPENSION, STEERING, COMPUTERS SYSTEM.  WARRANTY SHALL INCLUDE 7000 HOURS,  FIVE (5) YEARS, 100,000 MILES no DEDUCTIBLE.                                                                                                        
	
	
	

	CAB CHASSIS EXTENDED WARRANTY

EXTENDED WARRANTY SHALL INCLUDE THE COMPLETE CHASSIS, ENGINE AND OEM ATTACHED COMPONENTS, RADIATOR, FAN CLUTCH, IDLER PULLEYS, TRANSMISSION, AND SELECTOR CONTROLS, DRIVE LINES AND U-JOINTS, ELECTRICAL SYSTEM INCLUDING OEM WIRE HARNESS, ALTERNATOR, STARTER, DASH INSTRUMENTATION CONTROLS, COMPUTERS, AND STEERING SYSTEM. WARRANTY SHALL INCLUDE TOWING FOR FIVE (5) YEARS AND UP TO 100,000 MILES.

                                                                            $________________________

EXCEPTIONS TO THE SPECIFICATIONS 
EXCEPTIONS TO THE SPECIFICATIONS OF ANY ITEMS STATED HEREIN SHALL BE FULLY DESCRIBED, BY ITEM NUMBER IN WRITING BY THE CONTRACTOR IN THE SPACE PROVIDED BELOW:




LUBBOCK POWER & LIGHT

MINIMUM SPECIFICATIONS
CAB CHASSIS AND 12 YARD DUMP 
BODY WITH HYDRAULIC HOIST

SPEC #: 7412-722  

MAKE 


 MODEL 



IT IS THE INTENT OF THIS SPECIFICATION, REFERENCED DOCUMENTS, REQUIREMENTS AND CONDITIONS SECTIONS TO DESCRIBE MINIMUM PERFORMANCE REQUIREMENTS.  THE VEHICLE OR PRODUCT SHALL MEET OR EXCEED THE PERFORMANCE OR CONSTRUCTION DESCRIBED HEREIN. THE VENDOR SHALL BE REQUIRED TO MARK COMPLIANCE OR NON-COMPLIANCE TO EACH ITEM DESCRIPTION IN THE SPACE PROVIDED. ALL EQUIPMENT FURNISHED AS STANDARD TO THE GENERAL PUBLIC ON THE PRODUCT BY THE MANUFACTURER SHALL BE INCLUDED, EVEN WHEN NOT SPECIFICALLY IDENTIFIED IN THIS SPECIFICATION. ANY DEVIATIONS FROM THE WRITTEN SPECIFICATION WITH DATE AS SHOWN IN THE INVITATION TO BID (ITB) SHALL BE NOTED ON THE ATTACHED EXCEPTIONS TO THE SPECIFICATION. IN ORDER TO RECEIVE FULL CONSIDERATION, ITB RESPONSE QUOTATION MUST FOLLOW THIS SPECIFICATION AND THE INVITATION TO BID'S TERMS AND CONDITIONS.

NO.
ITEM

MINIMUM REQUIREMENTS
 SELLER COMPLIANCE


YES
NO


	
	EXCEPTIONS

	vendor EXCEPTIONS or additions shall be listed on the sheet provided at end of this bid. do list items on the bid itself
	
	
	

	
	SCOPE
	THIS SPECIFICATION DESCRIBES A DUMP BODY, OF 12.9 CUBIC YARD HEAPED CAPACITY, 10 YARD WATER LEVEL WITH HINGED TAIL GATE, AND HYDRAULIC HOISTING ASSEMBLY FURNISHED AND INSTALLED UPON ALL THREE AXLE CHASSIS
	
	
	

	1.
	DUMP BODY
	GALION #502 12.9 CU YD OR LP&L APPROVED EQUAL
	
	
	

	2.
	MODEL
	PACKAGE 96 OR LP&L APPROVED EQUAL
	
	
	

	3.
	DIMENSIONS
	LENGTH AND WIDTH: 180” L X 84” W
	
	
	

	4.
	HEAD/TAIL BOARD
	FRONT AND BACK: 38” ABOVE BODY FLOOR HEIGHTS
	
	
	

	5.
	TAILGATE
	AIR OPERATED INCLUDING HEAVY-DUTY GATE HINGES, WITH BOXED REAR CORNER POST WELDED FIRMLY AT ALL POINTS INCLUDING SIDE SHEET AND FLOOR
	
	
	

	6.
	HEIGHT ON SIDES
	31” METAL SIDES, WITH 6” CHANNEL SIDEBOARD EXTENSIONS
	
	
	

	7.
	BODY CAPACITY
	12.9 CUBIC YARDS HEAPED CAPACITY WITH SIDEBOARD EXTENSIONS
	
	
	

	8.
	PTO
	HOT SHIFT PTO, AIR OPERATED PTO ENGAGEMENT WITH CONTROLS MOUNTED CONVIENT TO OPERATOR’S REACH.
	
	
	

	9.
	HOIST
	GALION #63128 NTEA APPROVED CLASS 90 28.5 TON OR LP&L APPROVED EQUAL
	
	
	

	10.
	CYLINDER
	SHALL BE OF THE MULTI-STAGE  DESIGN WITH HOLDING FEATURE PREVENTING BED FALLING IN THE EVENT OF LINE FAILURE. CYLINDER SHALL BE LOCATED AT FRONT OF BODY WITH REMOVABLE ACCESS PANEL AT TOP OF HOIST.
	
	
	

	11.
	HYDRAULIC PUMP
	PUMP TO BE DIRECT DRIVE PTO MOUNTED. 
	
	
	

	12.
	HYDRAULIC RESERVOIR
	RESERVOIR SHALL BE GALION STANDARD CAPACITY, MOUNTED RESERVIOR SHALL BE EQUIPPED WITH A SHUT OFF VALVE CAPABLE OF SHUTTING OFF ALL FLOW FROM TANK.
	
	
	

	13.
	METAL  GAUGES   
	CONSTRUCTION ON SIDES:   8 GAUGE OR 10 GAUGE HIGH TENSILE WEAR RESISTANT METALS, FLOOR MATERIAL SHALL BE NOT LESS THAN 3/16  HIGH TENSILE AND WEAR RESISTANT AND HAVE A 2” FLOOR RADIUS
	
	
	

	14.
	MAIN FRAME
	TWO EACH 8” BEAM OR 7” CHANNEL LONGITUDINAL RAILS
	
	
	

	15.
	CROSS MEMBERS
	MINIMUM 4” HIGH CHANNEL AT NOT MORE THAN 24” CENTERS GUSSETED AND WELDED TO MAIN FRAME RAILS
	
	
	

	16.
	TAILGATE BRACES
	SLOPING TOP SURFACE AT EACH SIDE TO CONNECT TO SIDEBOADS
	
	
	

	17.
	CAB PROTECTION
	MINIMUM 1/2 CAB FULL WIDTH CAB PROTECTION
	
	
	

	18.
	UNDERCOATING
	DUMP BODY SHALL BE UNDERCOATED TO PREVENT RUST
	
	
	

	19.
	PAINT FINISH
	BODY AND ATTACHMENTS SHALL BE CLEANED PRIMED AND PAINTED WITH ACRYLIC ENAMEL OR POLY TYPE PAINT FINISH COLOR BLACK
	
	
	

	20.
	BUCK PLATE   
	THE REAR OF TRUCK SHALL BE PROVIDED WITH A HEAVY DUTY BUCK PLATE WITH THE FOLLOWING. TWO SAFETY RINGS, A SAE/ICC SIX (6) WAY FEMALE TRAILER PLUG, WIRED TO DOT GUIDELINES.  IF CAB CHASSIS CAME EQUIPPED WITH A 7-WAY PLUG IT TOO SHALL BE MOUNTED IN THE BUCK PLATE. 

 
	
	
	

	21.
	PINTLE  HITCH
	A holland PH-775SL  PINTLE HITCH MOUNTED TO THE BUCKBOARD AT THE HEIGHT OF AT LEAST 24 (+/-2”) INCHES AND BE BRACED TO FRAME OF the TRUCK. 
	
	
	

	22.
	LADDER
	THE DUMP BODY SHALL HAVE A LADDER ON THE DRIVERS SIDE WITH ONE STEP INSIDE BED FOR EASY ENTRY INTO BED  
	
	
	

	23.
	LIGHTS
	STOP/TAIL/TURN LIGHTS SHALL BE 4 INCH TRUCKLITE SUPER 44 LED IN A FLUSH SHOCK ABSORBING RUBBER ALL MARKER LIGHTS  SHALL ALSO BE LED TYPE.
 
	
	
	

	24.
	TOOLBOXES
	TWO, water tight TOOL Boxes 36” length, 20” depth, 

20” heighT.  CURB SIDE TO BE A DROP DOOR AND STREETSIDE

SHALL BE A SWING DOOR.  Tool boxes TO BOLT TO ¼” X 2”

ANGLE mounted TO FRAME OF TRUCK.  boxes SHALL BE painted black. brackets AND toolbox cannot be welded to frame. BOTH BOXE SHALL BE  DUTEC OR WEATHER GUARD


	
	
	


	
	TRUCK CHASSIS  SPEC
	
	
	
	

	1.
	 CHASSIS  
	 A THREE AXLE CHASSIS, 6 X 4 WITH A CONVENTIONAL CAB  
	
	
	

	2.
	WHEEL BASE
	cab CHASSIS TO TRUNION MEASURMENT WILL be DETERMINED BY VENDOR TO BE CORRECT LENGTH FOR BED BID.
	
	
	

	3.
	GVWR
	56,000 POUNDS
	
	
	

	4.
	FRONT AXLE
	SET BACK 12,000 POUNDS MINIMUM, WITH OIL TYPE HUBCAPS  WITH VIEW WINDOW
	
	
	

	5.
	REAR AXLE
	44,000 LB. TANDEM axle WITH DASH MOUNTED INTERLOCK CONTROLS. AXLES SHALL BE WALKING BEAM  SUSPENISION.         NO  AIR RIDE OR  T-TYPE  SUSPENISION                                                                                              
	
	
	

	6.
	AXLE RATIO
	Rear axle ratio should just provide max start and 2.5% at 65 mph fully loaded.
	
	
	

	7.
	SHOCKS
	MANUFACTURER’S FRONT AXLE, HEAVY DUTY SHOCKS.
	
	
	

	8.
	SPRINGS
	OEM SUSPENSION RATED FOR GVWR. 
	
	
	

	9.
	ENGINE
	HIGH  TORQUE DIESEL, RATED AT 300 HORSE  POWER WITH NOT LESS THAN  800 FT. LBS. TORQUE 
	
	
	

	10.
	EXHAUST
	SINGLE HORIZONTAL MUFFLER WITH HORIZONTAL TAIL PIPE SHALL BE  RIGHT-HAND MOUNTED 
	
	
	

	11.
	BLOCK- HEATER                       
	PHILLIPS-TEMRO 1000 WATT/115 VOLT BLOCK HEATER CHROME ENGINE HEATER RECEPTACLE MOUNTED UNDER LEFT HAND DOOR. sHALL HAVE A CORD TO PLUG INTO 120 VOLTS  
	
	
	

	12.
	TRANSMISSION
	TRANSMISSION SHALL BE A 6-SPEED ALLISON MODEL3500 RDS.  CONTROLS SHALL BE DASH MOUNTED 
	
	
	

	13.
	TIRES 
	11R X 22.5 RADIALS.  FRONT TIRES WITH HIGHWAY TREAD, MUD AND SNOW TREAD ON THE DRIVE AXLES.  ALL TIRES SHALL BE GOODYEAR TO LOWER REPLACMENT COST.
	
	
	

	14.
	WHEELS
	10-HOLE DISK TYPE, 22.5 X 8.25, TUBELESS
	
	
	

	15.
	BRAKES
	FULL AIR BRAKE SYSTEM CONFORMING TO DOT REQUIREMENTS, WITH OUTBOARD MOUNTED REAR BRAKE DRUMS.


	
	
	

	16.
	AIR DRYER
	THE AIR BRAKE SYSTEM SHALL BE FURNISHED WITH AUTOMATIC DRAIN VALVE ON THE WET TANK AND A HEATED AIR DRYER


	
	
	

	17.
	STEERING
	MANUFACTURER'S STANDARD POWER ASSISTED
	
	
	

	18.
	FUEL TANKS
	OEM DUAL STEP TANKS WITH NOT LESS THAN 80 GAL CAPACITY. 



	
	
	

	19.
	FRAME / BUMPER                   
	OEM double frame rated for sever duty SHALL BE CLEAR FROM BACK OF CAB TO REAR OF TRUCK.   BRACKETS AND SPRING HANGERS SHALL BE BOLTED. 
       
	
	
	

	20.
	INSTRUMENTS
	OEM FULL GAUGE INSTRUMENT DISPLAY TO INCLUDE ENGINE 

OIL PRESSURE, COOLANT TEMPERATURE, BATTERY CHARGE

INDICATOR, TACHOMETER AND ENGINE HOUR METER


	
	
	

	21.
	THROTTLE
	VERNIER LOCKING TYPE OR ELECTRICAL CONTROLLED HIGH

IDLE SPEED
	
	
	

	22.
	ALTERNATOR
	OEM HEAVY TRUCK TYPE ALTERNATOR WITH NOT LESS THAN 

160 AMP RATING.
	
	
	

	23.
	BATTERY
	DUAL 700 CCA FRAME MOUNTED WITH EXTERNAL POST FOR JUMP STARTING
	
	
	

	24.
	SEATS
	AIR RIDE SUSPENSION, high back WITH ARM REST ON BOTH

DRIVERS AND PASSENGERS SEATS  SHALL BE COVERED WITH

GRAY CLOTH.

	
	
	

	25.
	A/C, HEATER 
	OEM STANDARD AIR CONDITIONER/heating WITH DASH OUTLETS 
	
	
	

	26.
	MIRRORS
	HEATED, WEST COAST TYPE WITH A SEPARATELY MOUNTED convex type. one on each side
  
	
	
	

	27.
	GLAZING
	OEM  POWER WINDOWS WITH deep TINTED GLASS.  
	
	
	

	28.
	GRAB HANDLES
	OEM GRAB HANDLES, MOUNTED ON each side of  the CAB L&R

BEHIND DOORS
	
	
	

	29.
	12V-DC OUTLET
	TWO OEM STANDARD POWER OUTLETS INSIDE CAB .
	
	
	

	30.
	INTERIOR
	OEM DOME LIGHT WITH MAXIUM INSULATION PACKAGE WITH

AN INSULATED HEADLINER with SUN VISORS on both sides
	
	
	

	31.
	RADIO
	OEM AM/FM WITH TWO SPEAKERS AND CLOCK DISPLAY.
	
	
	

	32.
	WIPERS
	OEM 2 SPEED WITH INTERMITTENT FEATURE AND WASHERS
	
	
	

	33.
	HORNS
	OEM ELECTRIC AND AIR HORNS.  AIR HORNS TO BE MOUNTED 

UNDER HOOD
	
	
	

	34.
	Bumper
	FRONT BUMPER BE SHALL BE  ¼  THICK WITH SWEPT BACK ENDS. 
	
	
	

	35.
	BACKUP ALARM
	AN AUTOMATIC ACTING ELECTRIC BACKUP ALARM.
	
	
	

	36.
	TOW HOOKS
	TWO (2) EACH, TOW HOOKS OEM MOUNTED ON FRONT OF THE FRAME


	
	
	

	37.
	WIRING
	OEM WIRING SHALL BE ROUTED TO THE END OF THE FRAME FOR UPFITTERS USE.
	
	
	

	38.
	PAINT COLOR
	TRUCK SHALL BE OEM fleet WHITE COLOR WITH A BLACK FRAME. THE BED SHALL BE PREPAIRED, PRIMED AND PAINTED WITH BLACK

URETHANE PAINT. 


	
	
	

	39.
	 demonstration
	VENDOR MAY BE REQUIRED TO DO AN ONSITE demonstration OF UNIT AT NO COST TO LP&L FOR BID FOR ACCEPTANCE
	
	
	

	40.
	manufacturer’s print-out 
	Bidder shall provide a manufacturer’s print-out (Ford “DORA”/“Commerical Truck Tools”, Freightliner “Spec Pro”,   International “Vehicle Specifications”, Mack “Order/Customer/Vehicle Information”, or approved equivalent) to verify the vehicle bid meets all the requirements of this specification. Also, any dealer installed aftermarket components, if specified, must be noted                                                                                                   
	
	
	

	41.
	warranty
	all warrantIES shall have a Delay in warranty start date to allow for body installation. Warranty to become effective when vehicle is placed IN SERVICE BY LUBBOCK POWER & lIGHT rather than at time of delivery 
	
	
	


	42.
	DUMP BED WARRANTY
	THE DUMP BODY AND COMPONENTS OF THE HYDRAULIC SYSTEM CONTROLS AND THE INSTALLATION SHALL BE 100% WARRANTY PARTS AND LABOR FOR NOT LESS THAN 0NE (1) YEAR AFTER ACCEPTANCE BY LP&L.
	
	
	

	43.
	LITERATURE
	ALL manufacturer’s LITERATURE FOR BED, CAB CHASSIS AND EQUIPMENT SHALL BE ATTACHED TO THE BID 
	
	
	

	44.
	modificationS
	Welding shall not BE permitted on the frame side rails, nor shall the frame rails be cut to lengthen or shorten the wheelbase. Wheelbase modifications are allowed only by sliding the suspension with the “AF” dimension affected accordingly (excess length behind the rear axle may be cut off as required). Any wheelbase modification shall result in a wheelbase and frame combination that is identical to one available from the manufacturer. 
	
	
	

	 45.
	AUTHORIZED WARRANTY CENTER


	THE BIDDER SHALL BE  A FACTORY AUTHORIZED WARRANTY CENTER WITH COMPLETE PARTS,  SERVICE OF  CAB CHASSIS, DUMP BODY, COMPONENTS OF THE HYDRAULIC SYSTEM  AND CONTROLS 

BIDDER SHALL SUBMIT  PROOF  OF FACTORY AUTHORIZED SERVICE CENTER attached to bid ALONG WITH SPECIFICATION  SHEETS OFFERED IN RESPONSE TO SOLICITATION.   
	
	
	

	46.
	SERVICE CENTER
	if not an AUTHORIZED SERVICE CENTER LIST one in SPACE PROVIDED BELOW.

DEALER  NAME    ______________________________  

City                        __________________________________
MILEAGE              ______________________________ 

	
	
	

	47.
	MSO /  TITLE application
	 MSO / TITLE application SHALL BE MADE OUT TO THE CITY OF LUBBOCK. Vendor  shall ALSO certify the vehicle as a  completed unit.  DELIVER compeleted unit TO 402 MUNICIPAL DR. unit shall be delivered with a certified weight slip and four (4) set of keys.
	
	
	

	
	
	OPTIONS

	
	
	

	1.
	CAB CHASSIS  EXTENDED WARRANTY
	OEM manufacturer’s OEM EXTENDED WARRANTY SHALL INCLUDE THE COMPLETE CHASSIS, ENGINE AND OEM ATTACHED COMPONENTS, RADIATOR, FAN CLUTCH, IDLER PULLEYS, TRANSMISSION, AND SELECTOR CONTROLS, DRIVELINES AND U-JOINTS, ELECTRICAL SYSTEM INCLUDING OEM WIRE HARNESS, ALTERNATOR, STARTER, DASH INSTRUMENTATION AND CONTROLS, FULL SUSPENSION, STEERING, COMPUTERS SYSTEM.  WARRANTY SHALL INCLUDE 7000 HOURS, FIVE (5) YEARS, 100,000 MILES no DEDUCTIBLE.     
                            $_____________________________________________                                                                                                   
	
	
	

	EXCEPTIONS TO THE SPECIFICATIONS
EXCEPTIONS TO THE SPECIFICATIONS OF ANY ITEMS STATED HEREIN SHALL BE FULLY DESCRIBED, BY ITEM NUMBER IN WRITING BY THE CONTRACTOR IN THE SPACE PROVIDED BELOW:
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